output 1 momentary, Reply-STOP-to-opt-out
OUTPUT 1 M OK
output 1 hold open, Reply-STOP-to-opt-out
OUTPUT 1 HO OK
output 1 release, Reply-STOP-to-opt-out
OUTPUT 1 R OK

output 2 momentary, Reply-STOP-to-opt-out
OUTPUT 2 M OK
output 2 hold open, Reply-STOP-to-opt-out
OUTPUT 2 HO OK
output 2 release, Reply-STOP-to-opt-out
OUTPUT 2 R OK

send reboot, Reply-STOP-to-opt-out
REBOOT OK

get status, Reply-STOP-to-opt-out
replies back device status